eac3to v3.34
command line: D:\Tcl\work\BD3D2MK3D\toolset\eac3to.exe 00000.track_4352.Eng.dtsma 00000.track_4352.Eng.5.1.ac3 -640 -down6 -dcadec -progressnumbers -log=eac3to_convert_to_AC3.log
------------------------------------------------------------------------------
DTS Master Audio, 7.1 channels, 24 bits, 48kHz
(core: DTS, 5.1 channels, 1509kbps, 48kHz)
Decoding with libDcaDec DTS Decoder...
Mixing surround channels...
Remapping channels...
Encoding AC3 <640kbps> with libAften...
Creating file "00000.track_4352.Eng.5.1.ac3"...
Clipping detected, a 2nd pass will be necessary.  <WARNING>
Original audio track, L+R+BL+BR: max 24 bits, average 16 bits.
Original audio track, C+LFE+SL+SR: constant bit depth of 16 bits.
Processed audio track, L+R+SL+SR: max 24 bits, average 17 bits.
Processed audio track, C+LFE: constant bit depth of 16 bits.
Starting 2nd pass...
Decoding with libDcaDec DTS Decoder...
Mixing surround channels...
Remapping channels...
Encoding AC3 <640kbps> with libAften...
Applying -2.76dB gain...
Creating file "00000.track_4352.Eng.5.1.ac3"...
The processed audio track has a constant bit depth of 64 bits.
eac3to processing took 16 minutes, 44 seconds.
Done.
