*************************************************************************
* AACPlus v2 Encoder (using Winamp 5.57 enc_aacplus.dll and nscrt.dll)
* Coding Technologies encoder 8.0.3
* Build Jul 17 2010, 21:13:27
* NOTE!	enc_aacplus.dll & nscrt.dll must be in executable directory
*	get it from Winamp 5.x and plugins directory.
*************************************************************************
* Copyright (c)2005 Dmirty Alexandrov (dimzon541@gmail.com)
* Copyright (c)2004 Will Fisher (will.fisher@gmail.com)
* Modified by Bernd Niedergesaess to work with BASS (www.un4seen.com)
*************************************************************************

Usage:
	enc_aacPlus.exe <inputfile> <outputfile> [options]

Input/Output:
	<inputfile>      : WAV input file (use - to read from STDIN)
	                   (must be 8 or 16 bit PCM, 32000, 44100 or 48000 Hz)
	<outputfile>     : Bitstream output file (use - to write to STDOUT)
	                   To write MPEG4 ISO compilant .mp4/.m4a:
	                     libmp4v2.dll [from Winamp folder] must be in the same directory
	                     (mp4/m4a not possible, if STDOUT is selected)

Options:
	--br <bitrate>   : Set bitrate (CBR) in bps. Default is 128000
	--ps             : Enable Parametric Stereo
	                   (bitrates up to 56000, only with HE-AAC)
	--is             : Prefer Independed Stereo
	                   (disables Joint Stereo M/S coding)
	--dc             : Prefer Dual Channel
	--mono           : Encode as Mono
	--lc             : Encode as LC-AAC (default)
	                   (mono:8-16, stereo: 16-320, 6ch: 160-320 kbps)
	--he             : Encode as HE-AAC
	                   (mono:8-64, stereo: 16-128, 6ch: 96-213 kbps)
	--high           : Encode as HE-AAC+ with hight bitrates
	                   (mono:8-160, stereo: 96-256, 6ch: 8-256 kbps)
	--speech         : Tune for Speech
	--pns            : Enable Perceptual Noise Subsitution (PNS)
	--mpeg2aac       : Force MPEG2 AAC
	                   (instead of let the encoder choose)
	--mpeg4aac       : Force MPEG4 AAC
	                   (instead of let the encoder choose)
	--silent         : Set silent mode, no progress and other output
	--rawpcm <r c b> : Signal RAW PCM input intead of WAV
	         <r>     : Samplerate in Hz (32000, 44100 or 48000)
	         <c>     : Channels count (1 or 2 or 6)
	         <b>     : Bit's per sample (8 or 16, little-endian)

Examples:
	enc_aacPlus.exe input.wav out.aac --br 56000
	enc_aacPlus.exe input.wav out.m4a --br 32000 --he --mp4box
	enc_aacPlus.exe - - --br 128000 --high --silent --rawpcm 44100 2 16
