Demuxer s16le [PCM signed 16-bit little-endian]:
    Common extensions: sw.
s16le demuxer AVOptions:
-sample_rate       <int>        .D....  (from 0 to INT_MAX)
-channels          <int>        .D....  (from 0 to INT_MAX)

