Muxer mpegts [MPEG-TS (MPEG-2 Transport Stream)]:
    Common extensions: ts,m2t,m2ts,mts.
    Mime type: video/x-mpegts.
    Default video codec: mpeg2video.
    Default audio codec: mp2.
MPEGTS muxer AVOptions:
  -mpegts_transport_stream_id <int>        E..... Set transport_stream_id field. (from 1 to 65535)
  -mpegts_original_network_id <int>        E..... Set original_network_id field. (from 1 to 65535)
  -mpegts_service_id <int>        E..... Set service_id field. (from 1 to 65535)
  -mpegts_pmt_start_pid <int>        E..... Set the first pid of the PMT. (from 16 to 7936)
  -mpegts_start_pid  <int>        E..... Set the first pid. (from 256 to 3840)
  -mpegts_m2ts_mode  <int>        E..... Enable m2ts mode. (from -1 to 1)
  -muxrate           <int>        E..... (from 0 to INT_MAX)
  -pes_payload_size  <int>        E..... Minimum PES packet payload in bytes (from 0 to INT_MAX)
  -mpegts_flags      <flags>      E..... MPEG-TS muxing flags
     resend_headers               E..... Reemit PAT/PMT before writing the next packet
     latm                         E..... Use LATM packetization for AAC
  -resend_headers    <int>        E..... Reemit PAT/PMT before writing the next packet (from 0 to INT_MAX)
  -mpegts_copyts     <int>        E..... dont offset dts/pts (from -1 to 1)

