Demuxer rtsp [RTSP input]:
RTSP demuxer AVOptions:
-initial_pause     <int>        .D.... Don't start playing the stream immediately (from 0 to 1)
-rtsp_transport    <flags>      ED.... RTSP transport protocols
   udp                          ED.... UDP
   tcp                          ED.... TCP
   udp_multicast                .D.... UDP multicast
   http                         .D.... HTTP tunneling
-rtsp_flags        <flags>      .D.... RTSP flags
   filter_src                   .D.... Only receive packets from the negotiated peer IP
   listen                       .D.... Wait for incoming connections
-allowed_media_types <flags>      .D.... Media types to accept from the server
   video                        .D.... Video
   audio                        .D.... Audio
   data                         .D.... Data
-min_port          <int>        ED.... Minimum local UDP port (from 0 to 65535)
-max_port          <int>        ED.... Maximum local UDP port (from 0 to 65535)
-timeout           <int>        .D.... Maximum timeout (in seconds) to wait for incoming connections. -1 is infinite. Implies flag listen (from INT_MIN to INT_MAX)
-reorder_queue_size <int>        .D.... Number of packets to buffer for handling of reordered packets (from -1 to INT_MAX)

