Demuxer u32le [PCM unsigned 32-bit little-endian]:
u32le demuxer AVOptions:
  -sample_rate       <int>        .D....  (from 0 to INT_MAX)
  -channels          <int>        .D....  (from 0 to INT_MAX)

