//project X optional file
//user colour table definition for DVB subpictures, creating a .sup file, as a replacement of the internal remapping

//required entries of a table:
//table=list name
//model=final colour link depth of this table in bits (2, 4, 8) (means max. 4, 16, 256 paletized colours, best value depends on broadcasters std. table)
//0..x=ARGB (alpha,red,green,blue as 32bit uimsbf, 8bit each)  (undefined colour links are fully transparent)

//you can add as many tables you wish

table=SVT
model=4
0=0
1=FF101000
2=0
3=FF101010
4=FF101010
5=FF101010
6=FF101010
7=FF101010
8=FF101010
9=FF101010
10=FF101010
11=FF989898
12=FF989898
13=FF989898
14=FFDCDCDC
15=FFDCDCDC

table=NRK
model=4
0=0
1=D4101010
2=D4101010
3=D4101010
4=D4101010
5=D4101010
6=D4101010
7=D4101010
8=D4101010
9=D4101010
10=FF7C7C7C
11=FF7C7C7C
12=FF7C7C7C
13=FFDCDCDC
14=FFDCDCDC
15=FFDCDCDC

table=YLE
model=4
0=0
1=FF010101
2=FF010101
3=FF010101
4=FF010101
5=FF010101
6=FF010101
7=FF9C9C9C
8=FF9C9C9C
9=FFD0D0D0
10=FFD0D0D0
11=FFD0D0D0
12=FFD0D0D0
13=FFD0D0D0
14=FFD0D0D0
15=FFD0D0D0

table=C+Pol
model=2
0=0
1=FF101010
2=FFDCDCDC
3=FF9C9C9C

