
Syntax: x265 [options] infile [-o] outfile
    infile can be YUV or Y4M
    outfile is raw HEVC bitstream

Executable Options:
-h/--help                        Show this help text and exit
-V/--version                     Show version info and exit

Output Options:
-o/--output <filename>           Bitstream output file name
   --log-level <string>          Logging level: none error warning info debug full. Default info
   --no-progress                 Disable CLI progress reports
   --[no-]cu-stats               Enable logging stats about distribution of cu across all modes. Default disabled
   --csv <filename>              Comma separated log file, log level >= 3 frame log, else one line per run

Input Options:
   --input <filename>            Raw YUV or Y4M input file name. `-` for stdin
   --y4m                         Force parsing of input stream as YUV4MPEG2 regardless of file extension
   --fps <float|rational>        Source frame rate (float or num/denom), auto-detected if Y4M
   --input-res WxH               Source picture size [w x h], auto-detected if Y4M
   --input-depth <integer>       Bit-depth of input file. Default 8
   --input-csp <string>          Source color space: i420, i444 or i422, auto-detected if Y4M. Default: i420
-f/--frames <integer>            Maximum number of frames to encode. Default all
   --seek <integer>              First frame to encode
   --[no-]interlace <bff|tff>    Indicate input pictures are interlace fields in temporal order. Default progressive
   --dither                      Enable dither if downscaling to 8 bit pixels. Default disabled

Quality reporting metrics:
   --[no-]ssim                   Enable reporting SSIM metric scores. Default disabled
   --[no-]psnr                   Enable reporting PSNR metric scores. Default disabled

Profile, Level, Tier:
   --profile <string>            Enforce an encode profile: main, main10, mainstillpicture
   --level-idc <integer|float>   Force a minumum required decoder level (as '5.0' or '50')
   --[no-]high-tier              If a decoder level is specified, this modifier selects High tier of that level

Threading, performance:
   --threads <integer>           Number of threads for thread pool (0: detect CPU core count, default)
-F/--frame-threads <integer>     Number of concurrently encoded frames. 0: auto-determined by core count
   --[no-]wpp                    Enable Wavefront Parallel Processing. Default enabled
   --[no-]pmode                  Parallel mode analysis. Default disabled
   --[no-]pme                    Parallel motion estimation. Default disabled
   --[no-]asm <bool|int|string>  Override CPU detection. Default: auto

Presets:
-p/--preset <string>             Trade off performance for compression efficiency. Default medium
                                 ultrafast, superfast, veryfast, faster, fast, medium, slow, slower, veryslow, or placebo
-t/--tune <string>               Tune the settings for a particular type of source or situation:
                                 psnr, ssim, grain, zerolatency, fastdecode or cbr

Quad-Tree size and depth:
-s/--ctu <64|32|16>              Maximum CU size (WxH). Default 64
   --tu-intra-depth <integer>    Max TU recursive depth for intra CUs. Default 1
   --tu-inter-depth <integer>    Max TU recursive depth for inter CUs. Default 1

Analysis:
   --rd <0..6>                   Level of RD in mode decision 0:least....6:full RDO. Default 3
   --psy-rd <0..2.0>             Strength of psycho-visual rate distortion optimization, 0 to disable. Default 0.0
   --psy-rdoq <0..50.0>          Strength of psycho-visual optimization in quantization, 0 to disable. Default 0.0
   --[no-]early-skip             Enable early SKIP detection. Default disabled
   --[no-]fast-cbf               Enable early outs based on whether residual is coded. Default disabled
   --[no-]tskip-fast             Enable fast intra transform skipping. Default disabled
   --nr-intra <integer>          An integer value in range of 0 to 2000, which denotes strength of noise reduction in intra CUs. Default 0
   --nr-inter <integer>          An integer value in range of 0 to 2000, which denotes strength of noise reduction in inter CUs. Default 0

Coding tools:
-w/--[no-]weightp                Enable weighted prediction in P slices. Default enabled
   --[no-]weightb                Enable weighted prediction in B slices. Default disabled
   --[no-]cu-lossless            Consider lossless mode in CU RDO decisions. Default disabled
   --[no-]signhide               Hide sign bit of one coeff per TU (rdo). Default enabled
   --[no-]tskip                  Enable intra 4x4 transform skipping. Default disabled

Temporal / motion search options:
   --me <string>                 Motion search method dia hex umh star full. Default 1
-m/--subme <integer>             Amount of subpel refinement to perform (0:least .. 7:most). Default 2 
   --merange <integer>           Motion search range. Default 57
   --max-merge <1..5>            Maximum number of merge candidates. Default 2
   --[no-]rect                   Enable rectangular motion partitions Nx2N and 2NxN. Default disabled
   --[no-]amp                    Enable asymmetric motion partitions, requires --rect. Default disabled
   --[no-]temporal-mvp           Enable temporal MV predictors. Default enabled

Spatial / intra options:
   --[no-]strong-intra-smoothing Enable strong intra smoothing for 32x32 blocks. Default enabled
   --[no-]constrained-intra      Constrained intra prediction (use only intra coded reference pixels) Default disabled
   --[no-]b-intra                Enable intra in B frames in veryslow presets. Default disabled
   --[no-]fast-intra             Enable faster search method for angular intra predictions. Default disabled
   --rdpenalty <0..2>            penalty for 32x32 intra TU in non-I slices. 0:disabled 1:RD-penalty 2:maximum. Default 0

Slice decision options:
   --[no-]open-gop               Enable open-GOP, allows I slices to be non-IDR. Default enabled
-I/--keyint <integer>            Max IDR period in frames. -1 for infinite-gop. Default 250
-i/--min-keyint <integer>        Scenecuts closer together than this are coded as I, not IDR. Default: auto
   --no-scenecut                 Disable adaptive I-frame decision
   --scenecut <integer>          How aggressively to insert extra I-frames. Default 40
   --rc-lookahead <integer>      Number of frames for frame-type lookahead (determines encoder latency) Default 20
   --bframes <integer>           Maximum number of consecutive b-frames (now it only enables B GOP structure) Default 4
   --bframe-bias <integer>       Bias towards B frame decisions. Default 0
   --b-adapt <0..2>              0 - none, 1 - fast, 2 - full (trellis) adaptive B frame scheduling. Default 2
   --[no-]b-pyramid              Use B-frames as references. Default enabled
   --ref <integer>               max number of L0 references to be allowed (1 .. 16) Default 3
   --qpfile <string>             Force frametypes and QPs for some or all frames
                                 Format of each line: framenumber frametype QP
                                 QP is optional (none lets x265 choose). Frametypes: I,i,P,B,b.
                                 QPs are restricted by qpmin/qpmax.

Rate control, Adaptive Quantization:
   --bitrate <integer>           Target bitrate (kbps) for ABR (implied). Default 0
-q/--qp <integer>                QP for P slices in CQP mode (implied). --ipratio and --pbration determine other slice QPs
   --crf <float>                 Quality-based VBR (0-51). Default 28.0
   --[no-]lossless               Enable lossless: bypass transform, quant and loop filters globally. Default disabled
   --crf-max <float>             With CRF+VBV, limit RF to this value. Default 0.000000
                                 May cause VBV underflows!
   --crf-min <float>             With CRF+VBV, limit RF to this value. Default 0.000000
                                 this specifies a minimum rate factor value for encode!
   --vbv-maxrate <integer>       Max local bitrate (kbit/s). Default 0
   --vbv-bufsize <integer>       Set size of the VBV buffer (kbit). Default 0
   --vbv-init <float>            Initial VBV buffer occupancy (fraction of bufsize or in kbits). Default 0.90
   --pass                        Multi pass rate control.
                                   - 1 : First pass, creates stats file
                                   - 2 : Last pass, does not overwrite stats file
                                   - 3 : Nth pass, overwrites stats file
   --stats                       Filename for stats file in multipass pass rate control. Default x265_2pass.log
   --[no-]slow-firstpass         Enable a slow first pass in a multipass rate control mode. Default disabled
   --analysis-mode <string|int>  save - Dump analysis info into file, load - Load analysis buffers from the file. Default 0
   --analysis-file <filename>    Specify file name used for either dumping or reading analysis data.
   --aq-mode <integer>           Mode for Adaptive Quantization - 0:none 1:uniform AQ 2:auto variance. Default 1
   --aq-strength <float>         Reduces blocking and blurring in flat and textured areas (0 to 3.0). Default 1.00
   --[no-]cutree                 Enable cutree for Adaptive Quantization. Default enabled
   --ipratio <float>             QP factor between I and P. Default 1.40
   --pbratio <float>             QP factor between P and B. Default 1.30
   --qcomp <float>               Weight given to predicted complexity. Default 0.60
   --ratetol <float>             Degree of rate fluctuation that can be tolerated. Default 1.00
   --cbqpoffs <integer>          Chroma Cb QP Offset. Default 0
   --crqpoffs <integer>          Chroma Cr QP Offset. Default 0
   --scaling-list <string>       Specify a file containing HM style quant scaling lists or 'default' or 'off'. Default: off
   --lambda-file <string>        Specify a file containing replacement values for the lambda tables
                                 MAX_MAX_QP+1 floats for lambda table, then again for lambda2 table
                                 Blank lines and lines starting with hash(#) are ignored
                                 Comma is considered to be white-space

Loop filters (deblock and SAO):
   --[no-]deblock                Enable Deblocking Loop Filter, optionally specify tC:Beta offsets Default enabled
   --[no-]sao                    Enable Sample Adaptive Offset. Default enabled
   --[no-]sao-non-deblock        Use non-deblocked pixels, else right/bottom boundary areas skipped. Default disabled

VUI options:
   --sar <width:height|int>      Sample Aspect Ratio, the ratio of width to height of an individual pixel.
                                 Choose from 0=undef, 1=1:1("square"), 2=12:11, 3=10:11, 4=16:11,
                                 5=40:33, 6=24:11, 7=20:11, 8=32:11, 9=80:33, 10=18:11, 11=15:11,
                                 12=64:33, 13=160:99, 14=4:3, 15=3:2, 16=2:1 or custom ratio of <int:int>. Default 0
   --crop-rect <string>          Add 'left,top,right,bottom' to the bitstream-level cropping rectangle
   --overscan <string>           Specify whether it is appropriate for decoder to show cropped region: undef, show or crop. Default undef
   --videoformat <string>        Specify video format from undef, component, pal, ntsc, secam, mac. Default undef
   --range <string>              Specify black level and range of luma and chroma signals as full or limited Default limited
   --colorprim <string>          Specify color primaries from undef, bt709, bt470m, bt470bg, smpte170m,
                                 smpte240m, film, bt2020. Default undef
   --transfer <string>           Specify transfer characteristics from undef, bt709, bt470m, bt470bg, smpte170m,
                                 smpte240m, linear, log100, log316, iec61966-2-4, bt1361e, iec61966-2-1,
                                 bt2020-10, bt2020-12. Default undef
   --colormatrix <string>        Specify color matrix setting from undef, bt709, fcc, bt470bg, smpte170m,
                                 smpte240m, GBR, YCgCo, bt2020nc, bt2020c. Default undef
   --chromaloc <integer>         Specify chroma sample location (0 to 5). Default of 0

Bitstream options:
   --[no-]info                   Emit SEI identifying encoder and parameters. Default enabled
   --[no-]aud                    Emit access unit delimiters at the start of each access unit. Default disabled
   --[no-]hrd                    Enable HRD parameters signaling. Default disabled
   --[no-]repeat-headers         Emit SPS and PPS headers at each keyframe. Default disabled
   --hash <integer>              Decoded Picture Hash SEI 0: disabled, 1: MD5, 2: CRC, 3: Checksum. Default 0

Reconstructed video options (debugging):
-r/--recon <filename>            Reconstructed raw image YUV or Y4M output file name
   --recon-depth <integer>       Bit-depth of reconstructed raw image file. Defaults to input bit depth, or 8 if Y4M


Complete documentation may be found at http://x265.readthedocs.org/en/default/cli.html
