NVEncC (x64) 1.09 by rigaya, build Jul 13 2015 20:01:07
  avi reader: disabled
  avs reader: enabled
  vpy reader: enabled

Usage: NVEncC.exe [Options] -i <input file> -o <output file>

Input can be avs, raw YUV, YUV4MPEG2(y4m).
When Input is in raw format, fps, input-res is required.

Ouput format will be in raw H.264/AVC or H.265/HEVC ES.

Example:
  NVEncC -i "<avsfilename>" -o "<outfilename>"
  avs2pipemod -y4mp "<avsfile>" | NVEncC --y4m -i - -o "<outfilename>"

Options: 
-h,-? --help                      print help
   --help-ja                      print help in Japanese
   --help-en                      print help in English
-v,--version                      print version info
   --check-hw                     Check for NVEnc
   --check-features               Check for NVEnc Features
   --check-environment            Check for Environment Info

-i,--input <filename>             set input filename
-o,--output <filename>            set output filename

 Input formats (auto detected from extension of not set)
   --raw                          set input as raw format
   --y4m                          set input as y4m format
   --avs                          set input as avs format
   --vpy                          set input as vpy format
   --vpy-mt                       set input as vpy(mt) format

   --input-res <int>x<int>        set input resolution
   --crop <int>,<int>,<int>,<int> crop pixels from left,top,right,bottom
-f,--fps <int>/<int> or <float>   set framerate

-c,--codec <string>               set ouput codec
                                    h264 (or avc), h265 (or hevc)
   --profile <string>             set codec profile
                                    H.264: baseline, main, high(   --videoformat <string>         undef, ntsc, component, pal, secam, mac
                                   default: undef
   --colormatrix <string>         undef, auto, bt709, smpte170m, bt470bg
                                  smpte240m, YCgCo, fcc, GBR
                                   default: undef
   --colorprim <string>           undef, auto, bt709, smpte170m, bt470m
                                  bt470bg, smpte240m, film
                                   default: undef
   --transfer <string>            undef, auto, bt709, smpte170m, bt470m
                                  bt470bg, smpte240m, linear, log100, log316
                                   default: undef

H.265/HEVC
   --cu-max <int>                 set max CU size
   --cu-min  <int>                set min CU size
                                    8, 16, 32 are avaliable