# IntegerSSE

Integer SSE is a set of instructions found in most modern processors. IntegerSSE is an extension of MMX.

SSE: New commands present in P3, P4, newer Celerons, Athlon XP, MP.

Integer SSE: A subset of the SSE command set, mostly used for video processing. These instructions are also present in AMD Athlon (all versions), AMD Duron (all versions).

Integer SSE instructions:

`MASKMOVQ` mmreg1, mmreg2

`MOVNTQ` mem64, mmreg

`PAVGB` mmreg1, mmreg2

`PAVGB` mmreg, mem64

`PAVGW` mmreg1, mmreg2

`PAVGW` mmreg, mem64

`PEXTRW` reg32, mmreg, imm8

`PINSRW` mmreg, reg32, imm8

`PINSRW` mmreg, mem16, imm8

`PMAXSW` mmreg1, mmreg2

`PMAXSW` mmreg, mem64

`PMAXUB` mmreg1, mmreg2

`PMAXUB` mmreg, mem64

`PMINSW` mmreg1, mmreg2

`PMINSW` mmreg, mem64

`PMINUB` mmreg1, mmreg2

`PMINUB` mmreg, mem64

`PMOVMSKB` reg32, mmreg

`PMULHUW` mmreg1, mmreg2

`PMULHUW` mmreg, mem64

`PSADBW` mmreg1, mmreg2

`PSADBW` mmreg, mem64

`PSHUFW` mmreg1, mmreg2, imm8

`PSHUFW` mmreg, mem64, imm8

`PREFETCHNTA` mem8

`PREFETCHT0` mem8

`PREFETCHT1` mem8

`PREFETCHT2` mem8

`SFENCE`

Back to AssemblerOptimizing

$Date: 2014/10/27 22:04:54 $