VCEEncC (x64) 1.03 by rigaya, build Oct 24 2015 19:52:08
  avs reader:   enabled
  vpy reader:   enabled
Usage: VCEEncC [Options] -i <filename> -o <filename>

input can be avs, vpy, raw YUV or YUV4MPEG2(y4m) format.
when raw(default), fps, input-res are also necessary.

output format will be raw H.264/AVC ES.

Example:
  VCEEncC -i "<avsfilename>" -o "<outfilename>"
  avs2pipemod -y4mp "<avsfile>" | VCEEncC --y4m -i - -o "<outfilename>"

Options: 
-h,-? --help                    show help
-v,--version                    show version info

-i,--input-file <filename>      set input file name
-o,--output-file <filename>     set ouput file name

   --check-vce                  check for vce support on system.

 Input formats (will be estimated from extension if not set.)
   --raw                        set input as raw format
   --y4m                        set input as y4m format
   --avs                        set input as avs format
   --vpy                        set input as vpy format
   --vpy-mt                     set input as vpy format in multi-thread

   --input-res <int>x<int>      set input resolution
   --fps <int>/<int>            set input framerate
   --crop <int>,<int>,<int>,<int>
                                set crop pixels of left, up, right, bottom.

-u,--quality <string>           set quality preset
                                 balanced(default), fast, slow
   --cqp <int> or               encode in Constant QP, default 22:24:27
         <int>:<int>:<int>      set qp value for i:p:b frame
   --cbr <int>                  set bitrate in CBR mode (kbps)
   --vbr <int>                  set bitrate in VBR mode (kbps)
   --qp-max <int>               set max qp
   --qp-min <int>               set min qp
-b,--bframes <int>              set consecutive b frames (default: 0)
   --(no-)b-pyramid             enable b-pyramid feature
   --b-deltaqp <int>            set qp offset for non-ref b frames
   --bref-deltaqp <int>         set qp offset for ref b frames
   --max-bitrate <int>          set max bitrate (kbps) (default: 20000)
   --vbv-bufsize <int>          set vbv buffer size (kbps) (default: 20000)
   --slices <int>               set number of slices per frame (default: 1)
   --(no-)skip-frame            enable skip frame feature
   --motion-est                 set motion estimation precision
                                 full-pel, half-pel, q-pel(default)
   --gop-len <int>              set length of gop (default: auto)
   --log-level <int>            set log level
                                 error, warn, info(default), debug
